# Network Design Assignment

To properly enable the mail server the firewall will first need to be configured to allow the web traffic through the Antivirus will need to be configured for Mail server protection to guard against attacks like SPAM and DoD. All emails need to pass through the Email filter appliance before reaching the External IP address will need to have special NAT rules configured to direct the traffic to and from the mail server.